Command line options

Log continuous settings:
-LCMS,x	;Every x seconds
-LCMM,x	;Every x minutes
-LCM,1	;Every 1 minute on the minute
-LCM,5	;Every 5 minutes on the 1/12th hour
-LCM,10	;Every 10 minutes on the 1/6th hour
-LCM,15	;Every 15 minutes on the 1/4 hour
-LCM,30	;Every 30 minutes on the 1/2 hour
-LCM,60	;Every hour on the hour

-LCR     ;Start recording right away
-LCMIN   ;Minimize Application after Log continuous window starts up

-LCTH,x  ;Threshold setting in mpsas, 0.0=all readings get recorded
-LCGN,x  ;Select the name of the GoTo script, x is the name of the script (without extension), ex. default
-LCGRS   ;Run GoTo script then shut down when done
  
Select device settings:
-SEI,x	;Select Ethernet device where x = IP address
-SEM,x	;Select Ethernet device where x = MAC address
  
-SU     ;Find only USB devices
-SUC,x	;Select USB device where x = communication portname i.e. /dev/ttyUSB0
-SUI,x[,y...]	;Select USB device where x = ID number ex FTD12345, or multiple
                 IDs for LogContinuous with the first one being the priority set like:
                 -SUI,FTD12345,FTD33333,FTD55555
-DLRSS  ; DL Retreive Send Shutdown to be used in conjunction with -SUI option.
-DLRESS ; DL Retreive then Erase then Send Shutdown to be used in conjunction with -SUI option.

-N      ;Do not search for devices at startup. This cuts down startup time, the user must press the Find button to find devices
-P	;Start up plotter view
-DLR	;Startup DL retreive view

-TCA	;Start up Concatenate/Analyze tool
-TCM    ;Start up Cloud removal / Milky way position tool
-TCMR   ;Start up Cloud removal / Milky way position tool, and recall previous filename
